## Exp. 2 Design an LED Chaser

**Program:-**

void setup()

{

pinMode(12, OUTPUT);

pinMode(8,OUTPUT);

pinMode(5,OUTPUT);

}

void loop()

{

digitalWrite(12, HIGH);

delay(1000);

digitalWrite(12, LOW);

delay(100);

digitalWrite(8, HIGH);

delay(1000);

digitalWrite(8, LOW);

delay(100);

digitalWrite(5, HIGH);

delay(1000);

digitalWrite(5, LOW);

delay(50);

}